**Disposable helmet liner Specification**



TECHNICAL COMMITTEE REPRESENTATION

The following organizations were represented on the Technical Committee:

Moi university –Department of Industrial and Textile Engineering

National Industrial Training Authority (NITA)

Ministry of Industrialization and Trade

Kenknit Eldoret Ltd

Spinknit Nakuru Ltd

Technical University of Kenya(TUK)

Ministry of Health

RIVATEX

Spinknit Ltd Nakuru

Royele suits Ltd

Egerton University — Department of Applied Community Development Studies

Kantoor Brands Inc Ltd

Kenyatta University

Intertek

Weavers worth Ltd

Mount Kenya University

Mbagathi Hospital

Kenya Bureau of Standards — Secretariat

REVISION OF KENYA STANDARDS

In order to keep abreast of progress in industry, Kenya Standards shall be regularly reviewed. Suggestions for improvements to published standards, addressed to the Managing Director, Kenya Bureau of Standards, are welcome.

© Kenya Bureau of Standards, 2021

Copyright. Users are reminded that by virtue of Section 25 of the Copyright Act, Cap. 130 of 2001 of the Laws of Kenya, copyright subsists in all Kenya Standards and except as provided under Section 25 of this Act, no Kenya Standard produced by Kenya Bureau of Standards may be reproduced, stored in a retrieval system in any form or transmitted by any means without prior permission in writing from the Managing Director.

**Disposable helmet liner Specification**

|  |  |
| --- | --- |
| Kenya Bureau of Standards, Popo Road, Off Mombasa Road, P.O. Box 54974 - 00200, Nairobi, Kenya | |
|  | +254 020 6948000, + 254 722202137, + 254 734600471 |
|  | info@kebs.org |
|  | @KEBS\_ke |
|  | kenya bureau of standards (kebs) |

Foreword

This Kenya Standard was prepared by the Technical Committee on Readymade Garments under the guidance of the Standards Project Committee, and it is in accordance with the procedures of the Kenya Bureau of Standards.

Helmet liners protects helmet from sweat, stains and odour. This standard will protect the users from substandard disposable helmet liners.

In the preparation of this standard reference was made to the following documents:

KS 2933 surgical cap – Specification

Acknowledgement is made for the assistance received from these sources.

1. **SCOPE**

This Kenya Standard prescribes the minimum requirements for disposable helmet liners.

1. **Normative references**

The following referenced documents referred to in the text in such a way that some or all of their content constitutes requirements of this document. For dated references, only the edition cited applies. For undated references, the latest edition of the referenced document (including any amendments) applies.

KS 816-Methods for determination of absorbency of absorbent textile materials

KS ISO 1833 Textiles — Quantitative chemical analysis (relevant parts)

KS ISO 9073-1, Textiles — Test methods for nonwovens Part 1: Determination of mass per unit area

KS ISO 9073-4, Textiles — Test methods for nonwovens — Part 4: Determination of tear resistance

KS ISO 9073-15, Textiles - Test methods for nonwovens part 15: Determination of air permeability

KS ISO 9073-18, Textiles — Test methods for nonwovens Part 18: Determination of breaking strength and elongation of nonwoven materials using the grab tensile test

1. **TERMS AND DEFINITIONS**

For the purpose of this standard, the following definition apply

**3.1 Air Permeability**

Velocity of an air flow passing perpendicularly through a test specimen under a prescribed air pressure differential over a certain time period

*Note: Air permeability is expressed in litres per square centimeter per second (l/cm2.s), or any other equivalent unit*

**3.2 Absorption capacity**

Mass of liquid that is absorbed per unit mass of test piece

1. **REQUIREMENT**

4**.1 Materials**

**4.1.1 General**

All materials, dyes and chemicals used in the manufacture of disposable helmet liners shall not cause any undesirable effects to the skin.

**4.1.2 Securing mechanism**

The disposable helmet liners shall be fitted with an approximate securing mechanism that fits comfortably around the head of the wearer.

**4.2 Workmanship**

The disposable helmet liners shall be made with first class workmanship throughout and shall be free from defects that affect their appearance and/or serviceability, and free from marks spots or stains incurred in their manufacture.

**4.3 Performance requirements**

Disposable helmet liners shall comply with the performance requirements given in Table 1 when tested in accordance with the test methods prescribed therein.

Table  **— Performance requirements for disposable helmet liners**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S/N** | **Characteristic** | | **Requirement** | **Test method** |
|  | Absorption capacity, seconds | | Above 60 | KS 816 Method 2 |
|  | Air Permeability, l/cm2.s, min | | 0.015 | KS ISO 9073-15\* |
|  | Breaking Strength, N, min | Cross direction | 15 | KS ISO 9073-18 |
| Machine direction | 35 |
|  | Mass per unit area, g/m2 ,min | | 13 | KS ISO 9073-1 |
|  | Fiber composition | | 100% Polyolefin | KS ISO 1833 |
|  | Tearing strength, N, min | Cross direction | 6 | KS ISO 9073-4 |
| Machine direction | 17 take the lower value |
| \*use differential pressure of 100 Pa across the specimen (ISO 9327) | | | | |

4.3 **Restricted colorants**

If helmet liners are dyed, it shall be free from colorants listed in KS ISO 14632 parts 1 & 3 and KS ISO 16373-2 & 3. Dyestuffs shall be identified in accordance with KS ISO 16373-1.

**5. PACKAGING**

5.1 All disposable helmet liners shall be packaged in a suitable acceptable packaging material.

**6. LABELLING**

6.1 The following information in English shall be legibly and indelibly marked on the secondary packaging in which the disposable helmet liners is supplied

1. manufacturers name and address
2. country of manufacture
3. Number of units
4. The colour of the product
5. Instructions for use and disposal